3493Tektronix TDS 200 1000 2000 Series Acquire Continuous Waveform.vi
This example shows how to use autosetup and acquire a waveform on a single channel.

Connector Pane

Front Panel

Block Diagram

Express VI Configuration Information

	Write To Measurement File
Write To Measurement File
Writes data to a text-based measurement file (.lvm) or binary measurement file (.tdm).
--------------------

This Express VI is configured as follows:

Mode: Save to one file
Filename: C:\Documents and Settings\rupnik\Desktop\3493LBManual\channel 1.lvm
If a file already exists: 
Description: 

	Write To Measurement File2
Write To Measurement File
Writes data to a text-based measurement file (.lvm) or binary measurement file (.tdm).
--------------------

This Express VI is configured as follows:

Mode: Save to one file
Filename: C:\Documents and Settings\rupnik\Desktop\3493LBManual\channel2.lvm
If a file already exists: 
Description: 

	Time Delay
Time Delay
Inserts a time delay into the calling VI.
--------------------

This Express VI is configured as follows:

Delay Time: 1 s